|  |  |  |  |
| --- | --- | --- | --- |
| **Notes** | **New Specification** | **Old Specification** | **Spec No.** |
|  | - The proposed system should save automatically last at least 10 configuration changes on the device storage. | - The proposed system should save automatically last 50 configuration changes on the device storage. | 3.10 |
|  | - Native (agentless integration) Windows AD user napping (Single sign on capability) for at least 10,000 DC objects. | - Native (agentless integration) Windows AD user napping (Single sign on capability) for at least 64,000 DC objects. | 7.1.4 |
|  | - Syslog messages (remotely to centralized Syslog server) | - Syslog messages (locally in same device and remotely to centralized Syslog server) | 8.10.5 |
|  | - NGFW must have Sandboxing capability should be enabled on the firewall | - NGFW must have Machine-Learning driven engine to prevent unknown files in real-time without need to perform additional dynamic analysis (aka Sandboxing) | 8.17 |

* **الغاء البند رقم (1.4) من المواصفات الحالية**
* **الابقاء على باقي المواصفات كما هي دون أي تغيير كما وردت في العطاء سابقاً.**